# SPDX-License-Identifier: BSD-3-Clause
# Copyright(c) 2010-2014 Intel Corporation

#include "common_linuxapp"

CONFIG_RTE_MACHINE="native"

CONFIG_RTE_ARCH="i686"
CONFIG_RTE_ARCH_I686=y
CONFIG_RTE_ARCH_X86=y

CONFIG_RTE_TOOLCHAIN="gcc"
CONFIG_RTE_TOOLCHAIN_GCC=y

#
# KNI is not supported on 32-bit
#
CONFIG_RTE_LIBRTE_KNI=n

#
# Solarflare PMD is not supported on 32-bit
#
CONFIG_RTE_LIBRTE_SFC_EFX_PMD=n

#
# AES-NI multi-buffer PMD is not supported on 32-bit
#
CONFIG_RTE_LIBRTE_PMD_AESNI_MB=n

#
# AES-NI GCM PMD is not supported on 32-bit
#
CONFIG_RTE_LIBRTE_PMD_AESNI_GCM=n

#
# KASUMI PMD is not supported on 32-bit
#
CONFIG_RTE_LIBRTE_PMD_KASUMI=n

#
# ZUC PMD is not supported on 32-bit
#
CONFIG_RTE_LIBRTE_PMD_ZUC=n

#
# AVP PMD is not supported on 32-bit
#
CONFIG_RTE_LIBRTE_AVP_PMD=n

# 32-bit doesn't break up memory in lists, but does have VA allocation limit
CONFIG_RTE_MAX_MEM_MB=2048
